Bad Apple demo by NOBOMI for SHARP MZ-1500

This demo works in 40x25 TEXT mode. It uses 34x25
characters and PCG 8x8 pixels, so the resolution is
272x200 pixels, frame rate 20 fps. 2x256 PCG characters
are used for even and odd frames and only necessary changes
are redefined in PCG. Kind of RLE compression is used then.

This demo requires EMM disk with 4 MB capacity.
Use the file bad_apple_MZ1500.mze as EMM contents,
then run bad_apple_MZ.mzf. The executable is universal
for both MZ-800 and MZ-1500.

The EMM disk can be emulated eg. by Unicard. 
Some versions of Unicard Manager does not support
mounting EMM files, but Unicard firmware does, so please
set your EMM disk in emm.cfg file or use inglude manager.
Both files are included in unicard folder.

You can use TAKEDA, toshiya's EmuZ-1500 emulator to run 
the Bad Apple demo. Rename bad_apple_MZ1500.mze to emm.rom
and put it in the same directory as mz1500.exe. 
Change the extension of bad_apple_MZ.mzf to mzt and load it.

Video from demo can be seen at https://youtu.be/ZUXAV1h2Hzw

Video by Anira adapted for SHARP MZ-1500 and coded by NOBOMI.
Touhou theme music from Masayoshi Minoshima adapted 
to BBC Micro by INVERSE PHASE https://inversephase.bandcamp.com/.